

OCEAN HOUSE UNIT RENOVATION/CONSTRUCTION ( as of January 1, 2026)

Requirements
Use of bat insulation only
Windows and doors must match other units 
Removal of any concrete walls must be illustrated and accompanied by an engineer’s verification letter
Soundproofing for non-carpeted flooring using a minimum of 70 STC and recommend Proflex 250
Installation of FloLogic Water Leak Detection System
Waterproofing between concrete slab and floor covering on any exterior areas.

Prohibitions
No use of Icynene or blown insulation
Only electrical conduit, plumbing lines and AC ducts are allowed in any attic space available
No penetrations through slab or exterior walls. Pre-existing penetrations require minimum 2 hour firestop system.
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